**EIGRP CONFIGURATION**

1. Rename the 1st router as your First Name, 2nd router as your Last Name, 3rd router as your favorite fruit, and the 4th as your favorite course.
2. Configure the interface on both routers based on the described IPs on each interface
3. Configure statically each PC with a labeled IP address and its corresponding Gateway address
4. Configure the EIGRP routing protocol to enable all routers to communicate
5. Configure the passive-interface where necessary
6. Share the proof of communication among networks.

